Raspberry Program—Motion Capture& Remote web monitor

Additional Required Equipment:

USB Camera/ Raspberry Camera

Additional Software Requirement:

motion

Check if camera available:

Cd /dev

Is | grep video [vedio0, the index number increase if have multiple camera]

Set up motion:

Sudo apt-get update

Sudo apt-get install motion

Sudo nano /etc/motion/motion.conf

[confirm the image and video store location “target\_dir”]

Set “control\_loacalhost” to off

[allow remote device control http web console]

Before start remotely control motion, make sure motion is active at raspberry pi

&

Webcam\_localhost is off

http:8080

Motion Capture Video Type: swf